WMS-F-02  Rev 0 (DRAFT)
	Execution Specification
	WMS-F-02



Prepared per contract for BS EN 1090 work, from the technical review. It is the document that tells the shop floor what EXC2 actually requires on this job.
	Customer
	 
	IDM job no.
	 

	Structure / component
	 
	Drawing no. / rev
	 

	Execution Class
	EXC2
	Date
	 



	Requirement
	Specified for this contract

	Constituent products and grades
	 

	Material certification required
	3.1

	Cutting method and edge condition
	 

	Hole forming method
	 

	Weld preparation requirements
	 

	Welding processes permitted
	 

	WPS applicable
	 

	Weld quality level required
	[from the imperfection quality level standard — enter from the standard held]

	Extent and method of NDT
	 

	Geometrical tolerances — essential
	 

	Geometrical tolerances — functional
	 

	Mechanical fastening requirements
	 

	Surface preparation and protective treatment
	 

	Handling, storage and transport
	 

	Erection requirements, if applicable
	 

	Inspection and test plan reference
	 

	Customer-specified additions
	 



The requirements above are populated from BS EN 1090-2 for EXC2 and from the contract. Enter values from the current text of the standard — this template does not assert them.
	Role
	Name
	Signature
	Date

	Prepared by
	 
	 
	 

	RWC — approved
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