WMS-G-01  Rev 0 (DRAFT)
	Certification Level Determination Record
	WMS-G-01



Records how the BS EN 15085-2 Certification Level was determined for IDM's rail work. The level follows from the weld performance classes of the components — it is not chosen.
	Field
	Entry

	Rail product range
	 

	Customers
	Alstom

	Weld performance classes arising
	CP C2 evidenced on drawing 24308. Complete for the remainder of the range.

	Weld inspection classes arising
	CT 3 evidenced on drawing 24308. Complete for the remainder of the range.

	Standard used
	BS EN 15085-2 and BS EN 15085-3 — enter the editions held

	Customer imposition
	CL2 imposed in writing by Alstom, drawing 24308 (Class 22X grille cover), note 4. Referenced standard DTRF 150215 Rev J.

	CERTIFICATION LEVEL DETERMINED
	CL2, across the rail product range

	RWC competence required
	Comprehensive technical knowledge for CL2 — evidence outstanding (WMS-G-06)

	Date of determination
	 

	Review trigger
	Any enquiry indicating a weld performance class above the range covered by CL2



Drawing 24308 is stamped as an advanced copy for validation only. Confirm the released revision before this record is signed.
	Role
	Name
	Signature
	Date

	Determined by
	 
	 
	 

	RWC — approved
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