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Records monitoring of essential welding parameters during welding, where the technical review or the inspection and test plan requires it. Reference: IDM-FPC-WQM-001 Section 12.
	Customer
	 
	IDM job no.
	 

	Customer order no.
	 
	Drawing no. / rev
	 

	Component
	 
	Date
	 



	WPS reference
	 
	Welder ID
	 

	Weld ID(s)
	 
	Surveyed by
	 



Parameter monitoring
	Date
	Run
	Current (A)
	Voltage (V)
	Travel speed
	Pre-heat / interpass °C
	Gas flow
	Within WPS Y/N
	Initials

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 



Observations during welding
	Check
	Observation
	Action if not acceptable

	Cleaning between runs
	 
	 

	Shape and profile of runs
	 
	 

	Back-gouging carried out as specified
	 
	 

	Weld sequence followed
	 
	 

	Consumable handling and condition
	 
	 

	Distortion control measures
	 
	 

	Working conditions suitable
	 
	 

	Intermediate checks required by the ITP
	 
	 



Any parameter outside the WPS range stops welding on that joint and is referred to the RWC before work continues. Record the referral in the welding activity log.
	Role
	Name
	Signature
	Date

	Surveyed by
	 
	 
	 

	Welding Coordinator (internal)
	 
	 
	 

	RWC — reviewed
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