WMS-F-11  Rev 0 (DRAFT)
	FPC Review & Constancy of Performance Record
	WMS-F-11



Annual review that the factory production control system continues to deliver constancy of performance for the declared characteristics. Tabled alongside the welding management review (WMS-A-09).
	Review date
	 
	Prepared by
	 

	Period covered
	 
	Minute ref
	 



	Element reviewed
	Findings for the period
	Action required

	Execution Class determination still valid for the product range
	 
	 

	Execution specifications produced for every 1090 contract
	 
	 

	FPC 01–06 current and consistent with IDM-FPC-WQM-001
	 
	 

	Constituent product certification — completeness and traceability
	 
	 

	Dimensional and geometrical tolerance results
	 
	 

	Weld quality results against the required quality level
	 
	 

	Corrosion protection results, where in scope
	 
	 

	Mechanical fastening results, where in scope
	 
	 

	Equipment calibration status
	 
	 

	Declarations of Performance issued in the period
	 
	 

	Marking applied correctly and consistently with the DoP
	 
	 

	Notified / approved body surveillance findings
	 
	 

	Non-conformances affecting declared characteristics
	 
	 

	Changes to product range, process or personnel affecting FPC
	 
	 



	Conclusion — does the FPC system continue to deliver constancy of performance for the declared characteristics? State the basis.

	 

	 

	 



Complete only for products actually placed on the market. The elements above are a working list — confirm the required review content against the current text of BS EN 1090-1 before first use. [TBC]
	Role
	Name
	Signature
	Date

	Prepared by
	 
	 
	 

	RWC — approved
	 
	 
	 

	General Manager — approved
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