IDM Engineering (Chester) Ltd
Welding Management System  ·  IDM-FPC-WQM-001
Production and Inspection Records — BS EN 15085-5

	Field
	Detail

	Document reference
	WMS-G-05 · Rev 0 — DRAFT

	Owner
	CRGI Solutions Ltd

	Approval
	Responsible Welding Coordinator · General Manager (IDM)

	Standards
	BS EN ISO 3834-2 · BS EN 1090-1/-2 · BS EN 15085-2


What this is
BS EN 15085-5 governs the manufacturing and inspection documentation retained for welded railway components. This record indexes what the welding management system produces for a rail job, so that when the certification body asks which records exist and where they are, the answer is one page rather than a search.
What it does not do is assert which records BS EN 15085-5 requires, or for how long. The edition IDM holds of that standard is unverified (WMS-A-11), and CRGI will not transcribe requirements from a text it has not confirmed. Section 2 is therefore completed on receipt of the edition, and is blank until then. [TBC]
1.  Records the system produces for a rail job
These exist, are controlled, and are generated by running a job through the job pack. Each is a blank form master at 08 Blank Forms - Masters.
	Ref
	Record
	Raised at

	WMS-E-01
	Contract and technical review
	Enquiry, before the job is accepted

	WMS-E-02
	Weld map and welder allocation
	Job planning — links each joint to its procedure and welder

	WMS-E-04
	Weld log
	As welding proceeds

	WMS-E-05
	Inspection record — visual, dimensional and NDT call-off
	In process and on completion

	WMS-E-08
	Non-conformance, concession and weld repair
	On any departure

	WMS-E-09
	Material and consumable issue
	On issue to the job

	WMS-E-12
	Release and certificate of conformity
	Release

	WMS-E-15
	Weld surveillance sheet
	Coordination surveillance

	WMS-E-13
	Welding activity log
	Continuously — not per job


2.  Record set required by BS EN 15085-5
To be completed against the current text of BS EN 15085-5 once the edition held is verified. Where a required record has no counterpart in Section 1, that is a gap to be raised, not a cell to be filled with the nearest available form.
	Record required by the standard
	Satisfied by
	Retention
	Verified by / date

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	


Retention periods are deliberately blank here and in WMS-B-16 for the same reason. They follow from the current text of BS EN 15085-5 and BS EN 1090-1, and an unverified retention period in a controlled document is a defect an auditor finds.
3.  Weld performance class and inspection
The extent and method of inspection follow the weld performance class assigned to each joint under BS EN 15085-3, which is a design output, not a production decision. Where IDM holds design responsibility the class comes from IDM; where the customer specifies it, from the customer document.
	Field
	Entry

	Certification level in scope
	CL2, confirmed by IDM across the rail product range

	Customer-imposed class
	Alstom drawing 24308 (Class 22X) specifies CP C2 and weld inspection class CT 3

	Released drawing revision confirmed
	[outstanding — the copy held is stamped as an advanced copy for validation only]

	Weld performance classes for the range
	[to be assigned — see WMS-G-02 and WMS-G-03]

	Acceptance level (BS EN ISO 5817)
	[to be set per class from the current text — not asserted]


4.  Where the records are filed
1. Completed job records: filed against the job number, per the job pack.
1. Blank masters: 08 Blank Forms - Masters. Downloaded fresh each time — copying a completed form is how an obsolete revision spreads.
1. Standing records not tied to a job: the welding activity log (WMS-E-13) and the standing registers.
1. Where the record database is connected, job and register records are held there and exported on a schedule for retention.
5.  Completion of this record
	Action
	Owner
	Status

	Confirm the edition of BS EN 15085-5 held
	IDM
	Outstanding — WMS-A-11

	Complete Section 2 against that edition
	CRGI
	Follows the above

	Assign weld performance classes across the range
	RWC / design
	Outstanding

	Confirm the released revision of drawing 24308
	IDM
	Outstanding

	Accept this record
	Responsible Welding Coordinator
	Outstanding



Controlled record under IDM-FPC-WQM-001. Filed at 08 Blank Forms - Masters. Reviewed on any change of certification scope or standard edition.
